|  |  |  |
| --- | --- | --- |
| View Issue Details | | |
|  | | | | | |
| ID: | Category: | Severity: | Reproducibility: | Date Submitted: | Last Update: |
| 131 | [Flight Test] Electricity | minor | have not tried | 2016-10-04 16:23 | 2016-10-05 14:24 |
|  | | | | | |
| Reporter: |  | Platform: |  |  | |
| Assigned To: |  | OS: |  |  | |
| Priority: | P1 | OS Version: |  |  | |
| Status: | new | Product Version: |  |  | |
| Product Build: |  | Resolution: | @5@ |  | |
| Projection: | none |  |  |  | |
| ETA: | none | Fixed in Version: |  |  | |
|  |  | Target Version: |  |  | |
| Decision screening TF: |  | | | | |
| Defect detected on: |  | | | | |
| Operational limitation: |  | | | | |
| Detection date: | 2016-10-04 | | | | |
| DQI/e-logbook links: |  | | | | |
| Action Owner: |  | | | | |
| Analysis: |  | | | | |
| Long-term solution: |  | | | | |
| Conf managment link reference: |  | | | | |
| Helionix/EN7 PR ID: |  | | | | |
|  | | | | | |
| Summary: | [Coeur Electrique] Perte DMAP au dÃ©marrage moteur sur prise de parc | | | | |
| Description: | Investigations : lâ€™EN7 et la MOS sont alimentÃ©s sur du SHED2  ConsÃ©quence OpÃ©rationnelle | | | | |
| Steps To Reproduce: |  | | | | |
| Additional Information: |  | | | | |
| Attached Files: |  | | | | |
|  | | | | | |
| |  |  | | --- | --- | | Notes | | |  | | | |  | | --- | | (0000050) | |  | | 2016-10-05 14:24 | | |  | | --- | | 05/10: DÃ©cision projet Ã  prendre | | | | | | | |