|  |
| --- |
| View Issue Details  |
|  |
| ID:  | Category:  | Severity:  | Reproducibility:  | Date Submitted:  | Last Update:  |
| 131  | [Flight Test] Electricity  | minor  | have not tried  | 2016-10-04 16:23  | 2016-10-05 14:24  |
|  |
| Reporter:  |  | Platform:  |  |   |
| Assigned To:  |  | OS:  |  |   |
| Priority:  | P1  | OS Version:  |  |   |
| Status:  | new  | Product Version:  |  |   |
| Product Build:  |  | Resolution:  | @5@  |   |
| Projection:  | none  |    |    |   |
| ETA:  | none  | Fixed in Version:  |  |   |
|    |    | Target Version:  |  |   |
| Decision screening TF:  |  |
| Defect detected on:  |  |
| Operational limitation:  |  |
| Detection date:  | 2016-10-04  |
| DQI/e-logbook links:  |  |
| Action Owner:  |  |
| Analysis:  |  |
| Long-term solution:  |  |
| Conf managment link reference:  |  |
| Helionix/EN7 PR ID:  |  |
|  |
| Summary:  | [Coeur Electrique] Perte DMAP au dÃ©marrage moteur sur prise de parc  |
| Description:  | Investigations : lâ€™EN7 et la MOS sont alimentÃ©s sur du SHED2ConsÃ©quence OpÃ©rationnelle  |
| Steps To Reproduce:  |  |
| Additional Information:  |  |
| Attached Files:  |  |
|   |
|

|  |
| --- |
| Notes  |
|  |
|

|  |
| --- |
| (0000050)  |
|  |
| 2016-10-05 14:24     |

 |

|  |
| --- |
| 05/10: DÃ©cision projet Ã  prendre |

 |

 |